**Highlights**

* Built an automated NIPS platform for solution mixing, casting, and phase inversion.
* Used compression tests with automated analysis to quantify mechanical response.
* Validated workflow reliability and reproduced known parameter-property trends.
* Showed potential for AI‑driven closed‑loop membrane optimization and exploration.